ESB32 Algorithm

* open Arduino IDE
* Open File > Preferences
* click and "Manage the handling of additional plates" (<https://dl.espressif.com/dl/package_esp32_index.json>)
* Open tools > "Arduino Uno" board >board manager
* Find ESP 32
* install the ESP32
* Connect the ESB32 to USB cable
* Open tools > "Arduino Uno" board > ESP32 Arduino > choose ESP32 type
* Change port to "COM3"
* Program the code
* load the code